BW31xx – App Dock Software Instructions

Steps to Upgrade Firmware:

First, please check the Serial number on the baby monitor and confirm that it is included in the list below.

|  |  |
| --- | --- |
|  | SN Range |
| BW3101 | 3101H4R00001-3101H4R00505 |
| 3101J4R00506-3101J4R01010 |
| 3101L4R01011-3101L4R01515 |
| 3101A5R00001-3101A5R00505 |
| 3101C5R00506-3101C5R01010 |
|  | SN Range |
| BW3102 | 3102G4R00001～3102G4R00505 |
| 3102I4R00506～3102I4R01010 |
| 3102J4R01011～3102J4R01515 |
| 3102K4R01516～3102K4R02020 |
| 3102L4R02021～3102L4R02525 |
| 3102A5R00001～3102A5R00505 |

After having confirmed the S/N of the unit, follow the steps below:

1)     Unzip the folder and copy the (.bin) file to a formatted micro SD card.

2)     Insert the micro SD card, power on the BW31xx monitor and press the PLAY/RECORD button.

3)     Next, press and hold both the "ZOOM" and "TALK" button, until *UBR243.bin* displays on the screen.

4)     Press OK to select the file and upgrade firmware.  Please wait until the display shows, “*UPDATE DONE! PLEASE RESTART SYSTEM*”.

5)     Power off the unit and take out the microSD card.

6)     Please pair the camera to the monitor once again (refer Owner’s Manual for pairing details).