**DFR6NZ / DFR7NZ PC UPDATE**

**INSTALL USB DRIVER TO YOUR PC**

1. Install USB driver (CP210xVCP) to your PC.
2. Open up the CP210x\_VCP\_Windows folder & select one of the two Applications.
3. CP210xVCPInstaller\_x64 for 64-bit Operating Systems.

OR

CP210xVCPInstaller\_x86 for 32-bit Operating Systems.

**FIRMWARE (DFR6NZ)**

1. Open up the DFR6\_NZ\_FW\_Update folder, and then select DFR6NZ\_FW\_Update\_Manager
2. Connect DFR6NZ to PC with a USB cable. The current version of Firmware will appear on the application.
3. Browse and select the file to update and start.

**FIRMWARE (DFR7NZ)**

1. Open up the DFR7\_NZ\_FW\_Update folder, and then select DFR7NZ\_FW\_Update\_Manager
2. Connect DFR7NZ to PC with a USB cable. The current version of Main Firmware and Sub (GPS) Firmware will appear on the application.
3. Browse and select the Main file to update and start.
4. Browse and select the Sub (GPS) file to update and start.

**SPEED CAMERA DATABASE (DFR7NZ ONLY)**

.

1. Open up the DFR7\_NZ\_DB\_Update folder, and then select DFR7NZ\_DB\_Update\_Manager
2. Connect DFR7NZ to PC with a USB cable. The current version of Database will appear on the application.
3. Browse and select the Database (DB) file to update and start.